中文说明:
HCAL色彩校正软件是运行在Windows操作系统上的照度计/亮度计的色彩校正软件,支持800系列分光辐照照度计,500系列色彩照度计,300系列色彩照度计,以及多种型号的亮度计和色彩分析仪。
采用滤光片探测器测试原理的照度计/亮度计通常会存在CIEXYZ适配误差，会导致该类型的照度计/亮度计的测试精度和数据一致性略差。
在这种情况下，可以对该类型的照度计/亮度计用HCAL软件进行校正，如果校正合理，与标准机测试数据对比，校正后的照度计/亮度计通常亮度精度可以达到3%、平均色品坐标xy误差在0.003。
注意1:HCAL支持Win10/Win11及以上版本操作系统.
注意2:HCAL支持直接通过Excel表格导入标准机和待校机数据.
注意3:HUICOLOR各种型号的照度计和亮度计均支持二次开发，有二次开发需求的用户可以找客服提供开发SDK及Demo。
--------------------------------------------------------------------
Description:
HCAL is a color calibration software for irradiance/ luminance colorimeter running on the Windows operating system. It supports 800 series spectral Irradiance Colorimeter, 500 series Irradiance Colorimeter, 300 series Irradiance Colorimeter, as well as various models of luminance colorimeter and color analyzers.
The testing principle of irradiance/ luminance colorimeter using coated filter plates+CMOS/PD silicon photovoltaic cell detectors usually has CIEXYZ adaptation errors, which can result in slightly lower testing accuracy and data consistency for this type of irradiance/ luminance colorimeter.
In this case, HCAL software can be used to calibrate this type of irradiance/ luminance colorimeter. If the calibration is reasonable and compared with standard machine test data, the calibrated irradiance/ luminance colorimeter usually has a luminance accuracy of 3% and an average chromaticity coordinate xy error of 0.003.
Note 1: HCAL supports Win10/Win11 and above operating systems.
Note 2: HCAL software supports direct import of standard colorimeter and test colorimeter  data through Excel sheets.
Note 3: HUICOROR's various models of illuminance and luminance meters support secondary development. Users with secondary development needs can contact customer service to provide development SDKs and demos.